make -f nbproject/Makefile-PRO_Comparison.mk SUBPROJECTS= .clean-conf
make[1]: Entering directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
rm -f  -r .ca/build/PRO_Comparison/production
rm -f  -r .ca/dist/PRO_Comparison/production
make[1]: Leaving directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
[32mCLEAN SUCCESSFUL (total time: 254ms)[0m
make -f nbproject/Makefile-PRO_Comparison.mk SUBPROJECTS= .build-conf
make  -f nbproject/Makefile-PRO_Comparison.mk .ca/dist/PRO_Comparison/production/PWM_LCD_AD_prj.X.production.hex
make[2]: Entering directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
"C:\Program Files\Microchip\xc8\v3.10\bin\xc8-cc.exe"  -mcpu=18F46K22 -c   -mdfp="C:/Program Files/Microchip/MPLABX/v6.30/packs/Microchip/PIC18F-K_DFP/1.15.303/xc8"  -memi=wordwrite -O0 -fasmfile -maddrqual=ignore -xassembler-with-cpp -mwarn=-3 -Wa,-a -DXPRJ_PRO_Comparison=PRO_Comparison  -msummary=-psect,-class,+mem,-hex,-file  -ginhx32 -Wl,--data-init -mno-keep-startup -mno-download -mno-default-config-bits   -std=c99 -gcoff -mstack=compiled:auto:auto:auto -Xparser -Wno-implicit-int-float-conversion  -Wno-implicit-int-conversion -Wno-#warnings -mafrlcsj     -o .ca/build/PRO_Comparison/production/mcc_generated_files/system/src/interrupt.p1 mcc_generated_files/system/src/interrupt.c 
make[2]: Leaving directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
make[2]: Entering directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
"C:\Program Files\Microchip\xc8\v3.10\bin\xc8-cc.exe"  -mcpu=18F46K22 -c   -mdfp="C:/Program Files/Microchip/MPLABX/v6.30/packs/Microchip/PIC18F-K_DFP/1.15.303/xc8"  -memi=wordwrite -O0 -fasmfile -maddrqual=ignore -xassembler-with-cpp -mwarn=-3 -Wa,-a -DXPRJ_PRO_Comparison=PRO_Comparison  -msummary=-psect,-class,+mem,-hex,-file  -ginhx32 -Wl,--data-init -mno-keep-startup -mno-download -mno-default-config-bits   -std=c99 -gcoff -mstack=compiled:auto:auto:auto -Xparser -Wno-implicit-int-float-conversion  -Wno-implicit-int-conversion -Wno-#warnings -mafrlcsj     -o .ca/build/PRO_Comparison/production/mcc_generated_files/adc/src/adc.p1 mcc_generated_files/adc/src/adc.c 
make[2]: Leaving directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
make[2]: Entering directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
"C:\Program Files\Microchip\xc8\v3.10\bin\xc8-cc.exe"  -mcpu=18F46K22 -c   -mdfp="C:/Program Files/Microchip/MPLABX/v6.30/packs/Microchip/PIC18F-K_DFP/1.15.303/xc8"  -memi=wordwrite -O0 -fasmfile -maddrqual=ignore -xassembler-with-cpp -mwarn=-3 -Wa,-a -DXPRJ_PRO_Comparison=PRO_Comparison  -msummary=-psect,-class,+mem,-hex,-file  -ginhx32 -Wl,--data-init -mno-keep-startup -mno-download -mno-default-config-bits   -std=c99 -gcoff -mstack=compiled:auto:auto:auto -Xparser -Wno-implicit-int-float-conversion  -Wno-implicit-int-conversion -Wno-#warnings -mafrlcsj     -o .ca/build/PRO_Comparison/production/mcc_generated_files/i2c_host/src/mssp2.p1 mcc_generated_files/i2c_host/src/mssp2.c 
make[2]: Leaving directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
make[2]: Entering directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
"C:\Program Files\Microchip\xc8\v3.10\bin\xc8-cc.exe"  -mcpu=18F46K22 -c   -mdfp="C:/Program Files/Microchip/MPLABX/v6.30/packs/Microchip/PIC18F-K_DFP/1.15.303/xc8"  -memi=wordwrite -O0 -fasmfile -maddrqual=ignore -xassembler-with-cpp -mwarn=-3 -Wa,-a -DXPRJ_PRO_Comparison=PRO_Comparison  -msummary=-psect,-class,+mem,-hex,-file  -ginhx32 -Wl,--data-init -mno-keep-startup -mno-download -mno-default-config-bits   -std=c99 -gcoff -mstack=compiled:auto:auto:auto -Xparser -Wno-implicit-int-float-conversion  -Wno-implicit-int-conversion -Wno-#warnings -mafrlcsj     -o .ca/build/PRO_Comparison/production/mcc_generated_files/system/src/system.p1 mcc_generated_files/system/src/system.c 
make[2]: Leaving directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
make[2]: Entering directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
"C:\Program Files\Microchip\xc8\v3.10\bin\xc8-cc.exe"  -mcpu=18F46K22 -c   -mdfp="C:/Program Files/Microchip/MPLABX/v6.30/packs/Microchip/PIC18F-K_DFP/1.15.303/xc8"  -memi=wordwrite -O0 -fasmfile -maddrqual=ignore -xassembler-with-cpp -mwarn=-3 -Wa,-a -DXPRJ_PRO_Comparison=PRO_Comparison  -msummary=-psect,-class,+mem,-hex,-file  -ginhx32 -Wl,--data-init -mno-keep-startup -mno-download -mno-default-config-bits   -std=c99 -gcoff -mstack=compiled:auto:auto:auto -Xparser -Wno-implicit-int-float-conversion  -Wno-implicit-int-conversion -Wno-#warnings -mafrlcsj     -o .ca/build/PRO_Comparison/production/mcc_generated_files/system/src/clock.p1 mcc_generated_files/system/src/clock.c 
make[2]: Leaving directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
make[2]: Entering directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
"C:\Program Files\Microchip\xc8\v3.10\bin\xc8-cc.exe"  -mcpu=18F46K22 -c   -mdfp="C:/Program Files/Microchip/MPLABX/v6.30/packs/Microchip/PIC18F-K_DFP/1.15.303/xc8"  -memi=wordwrite -O0 -fasmfile -maddrqual=ignore -xassembler-with-cpp -mwarn=-3 -Wa,-a -DXPRJ_PRO_Comparison=PRO_Comparison  -msummary=-psect,-class,+mem,-hex,-file  -ginhx32 -Wl,--data-init -mno-keep-startup -mno-download -mno-default-config-bits   -std=c99 -gcoff -mstack=compiled:auto:auto:auto -Xparser -Wno-implicit-int-float-conversion  -Wno-implicit-int-conversion -Wno-#warnings -mafrlcsj     -o .ca/build/PRO_Comparison/production/mcc_generated_files/system/src/config_bits.p1 mcc_generated_files/system/src/config_bits.c 
make[2]: Leaving directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
make[2]: Entering directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
"C:\Program Files\Microchip\xc8\v3.10\bin\xc8-cc.exe"  -mcpu=18F46K22 -c   -mdfp="C:/Program Files/Microchip/MPLABX/v6.30/packs/Microchip/PIC18F-K_DFP/1.15.303/xc8"  -memi=wordwrite -O0 -fasmfile -maddrqual=ignore -xassembler-with-cpp -mwarn=-3 -Wa,-a -DXPRJ_PRO_Comparison=PRO_Comparison  -msummary=-psect,-class,+mem,-hex,-file  -ginhx32 -Wl,--data-init -mno-keep-startup -mno-download -mno-default-config-bits   -std=c99 -gcoff -mstack=compiled:auto:auto:auto -Xparser -Wno-implicit-int-float-conversion  -Wno-implicit-int-conversion -Wno-#warnings -mafrlcsj     -o .ca/build/PRO_Comparison/production/mcc_generated_files/pwm/src/ccp5.p1 mcc_generated_files/pwm/src/ccp5.c 
make[2]: Leaving directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
make[2]: Entering directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
"C:\Program Files\Microchip\xc8\v3.10\bin\xc8-cc.exe"  -mcpu=18F46K22 -c   -mdfp="C:/Program Files/Microchip/MPLABX/v6.30/packs/Microchip/PIC18F-K_DFP/1.15.303/xc8"  -memi=wordwrite -O0 -fasmfile -maddrqual=ignore -xassembler-with-cpp -mwarn=-3 -Wa,-a -DXPRJ_PRO_Comparison=PRO_Comparison  -msummary=-psect,-class,+mem,-hex,-file  -ginhx32 -Wl,--data-init -mno-keep-startup -mno-download -mno-default-config-bits   -std=c99 -gcoff -mstack=compiled:auto:auto:auto -Xparser -Wno-implicit-int-float-conversion  -Wno-implicit-int-conversion -Wno-#warnings -mafrlcsj     -o .ca/build/PRO_Comparison/production/mcc_generated_files/system/src/pins.p1 mcc_generated_files/system/src/pins.c 
make[2]: Leaving directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
make[2]: Entering directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
"C:\Program Files\Microchip\xc8\v3.10\bin\xc8-cc.exe"  -mcpu=18F46K22 -c   -mdfp="C:/Program Files/Microchip/MPLABX/v6.30/packs/Microchip/PIC18F-K_DFP/1.15.303/xc8"  -memi=wordwrite -O0 -fasmfile -maddrqual=ignore -xassembler-with-cpp -mwarn=-3 -Wa,-a -DXPRJ_PRO_Comparison=PRO_Comparison  -msummary=-psect,-class,+mem,-hex,-file  -ginhx32 -Wl,--data-init -mno-keep-startup -mno-download -mno-default-config-bits   -std=c99 -gcoff -mstack=compiled:auto:auto:auto -Xparser -Wno-implicit-int-float-conversion  -Wno-implicit-int-conversion -Wno-#warnings -mafrlcsj     -o .ca/build/PRO_Comparison/production/mcc_generated_files/timer/src/tmr2.p1 mcc_generated_files/timer/src/tmr2.c 
make[2]: Leaving directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
make[2]: Entering directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
"C:\Program Files\Microchip\xc8\v3.10\bin\xc8-cc.exe"  -mcpu=18F46K22 -c   -mdfp="C:/Program Files/Microchip/MPLABX/v6.30/packs/Microchip/PIC18F-K_DFP/1.15.303/xc8"  -memi=wordwrite -O0 -fasmfile -maddrqual=ignore -xassembler-with-cpp -mwarn=-3 -Wa,-a -DXPRJ_PRO_Comparison=PRO_Comparison  -msummary=-psect,-class,+mem,-hex,-file  -ginhx32 -Wl,--data-init -mno-keep-startup -mno-download -mno-default-config-bits   -std=c99 -gcoff -mstack=compiled:auto:auto:auto -Xparser -Wno-implicit-int-float-conversion  -Wno-implicit-int-conversion -Wno-#warnings -mafrlcsj     -o .ca/build/PRO_Comparison/production/mcc_generated_files/timer/src/tmr0.p1 mcc_generated_files/timer/src/tmr0.c 
make[2]: Leaving directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
make[2]: Entering directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
"C:\Program Files\Microchip\xc8\v3.10\bin\xc8-cc.exe"  -mcpu=18F46K22 -c   -mdfp="C:/Program Files/Microchip/MPLABX/v6.30/packs/Microchip/PIC18F-K_DFP/1.15.303/xc8"  -memi=wordwrite -O0 -fasmfile -maddrqual=ignore -xassembler-with-cpp -mwarn=-3 -Wa,-a -DXPRJ_PRO_Comparison=PRO_Comparison  -msummary=-psect,-class,+mem,-hex,-file  -ginhx32 -Wl,--data-init -mno-keep-startup -mno-download -mno-default-config-bits   -std=c99 -gcoff -mstack=compiled:auto:auto:auto -Xparser -Wno-implicit-int-float-conversion  -Wno-implicit-int-conversion -Wno-#warnings -mafrlcsj     -o .ca/build/PRO_Comparison/production/_ext/1472/PWM_LCD_AD.p1 ../PWM_LCD_AD.c 
make[2]: Leaving directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
make[2]: Entering directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
"C:\Program Files\Microchip\xc8\v3.10\bin\xc8-cc.exe"  -mcpu=18F46K22 -c   -mdfp="C:/Program Files/Microchip/MPLABX/v6.30/packs/Microchip/PIC18F-K_DFP/1.15.303/xc8"  -memi=wordwrite -O0 -fasmfile -maddrqual=ignore -xassembler-with-cpp -mwarn=-3 -Wa,-a -DXPRJ_PRO_Comparison=PRO_Comparison  -msummary=-psect,-class,+mem,-hex,-file  -ginhx32 -Wl,--data-init -mno-keep-startup -mno-download -mno-default-config-bits   -std=c99 -gcoff -mstack=compiled:auto:auto:auto -Xparser -Wno-implicit-int-float-conversion  -Wno-implicit-int-conversion -Wno-#warnings -mafrlcsj     -o .ca/build/PRO_Comparison/production/PCF8574.p1 PCF8574.c 
make[2]: Leaving directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
make[2]: Entering directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
"C:\Program Files\Microchip\xc8\v3.10\bin\xc8-cc.exe"  -mcpu=18F46K22 -c   -mdfp="C:/Program Files/Microchip/MPLABX/v6.30/packs/Microchip/PIC18F-K_DFP/1.15.303/xc8"  -memi=wordwrite -O0 -fasmfile -maddrqual=ignore -xassembler-with-cpp -mwarn=-3 -Wa,-a -DXPRJ_PRO_Comparison=PRO_Comparison  -msummary=-psect,-class,+mem,-hex,-file  -ginhx32 -Wl,--data-init -mno-keep-startup -mno-download -mno-default-config-bits   -std=c99 -gcoff -mstack=compiled:auto:auto:auto -Xparser -Wno-implicit-int-float-conversion  -Wno-implicit-int-conversion -Wno-#warnings -mafrlcsj     -o .ca/build/PRO_Comparison/production/I2C_LCD.p1 I2C_LCD.c 
make[2]: Leaving directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
make[2]: Entering directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
"C:\Program Files\Microchip\xc8\v3.10\bin\xc8-cc.exe"  -mcpu=18F46K22 -Wl,-Map=.ca/dist/PRO_Comparison/production/PWM_LCD_AD_prj.X.production.map  -DXPRJ_PRO_Comparison=PRO_Comparison  -Wl,--defsym=__MPLAB_BUILD=1   -mdfp="C:/Program Files/Microchip/MPLABX/v6.30/packs/Microchip/PIC18F-K_DFP/1.15.303/xc8"  -memi=wordwrite -O0 -fasmfile -maddrqual=ignore -xassembler-with-cpp -mwarn=-3 -Wa,-a -msummary=-psect,-class,+mem,-hex,-file  -ginhx32 -Wl,--data-init -mno-keep-startup -mno-download -mno-default-config-bits -Xparser -Wno-implicit-int-float-conversion  -Wno-implicit-int-conversion -Wno-#warnings -mafrlcsj -std=c99 -gcoff -mstack=compiled:auto:auto:auto      -Wl,--memorysummary,.ca/dist/PRO_Comparison/production/memoryfile.xml -o .ca/dist/PRO_Comparison/production/PWM_LCD_AD_prj.X.production.elf  .ca/build/PRO_Comparison/production/mcc_generated_files/adc/src/adc.p1 .ca/build/PRO_Comparison/production/mcc_generated_files/i2c_host/src/mssp2.p1 .ca/build/PRO_Comparison/production/mcc_generated_files/pwm/src/ccp5.p1 .ca/build/PRO_Comparison/production/mcc_generated_files/system/src/interrupt.p1 .ca/build/PRO_Comparison/production/mcc_generated_files/system/src/clock.p1 .ca/build/PRO_Comparison/production/mcc_generated_files/system/src/system.p1 .ca/build/PRO_Comparison/production/mcc_generated_files/system/src/config_bits.p1 .ca/build/PRO_Comparison/production/mcc_generated_files/system/src/pins.p1 .ca/build/PRO_Comparison/production/mcc_generated_files/timer/src/tmr2.p1 .ca/build/PRO_Comparison/production/mcc_generated_files/timer/src/tmr0.p1 .ca/build/PRO_Comparison/production/PCF8574.p1 .ca/build/PRO_Comparison/production/_ext/1472/PWM_LCD_AD.p1 .ca/build/PRO_Comparison/production/I2C_LCD.p1     

    Program space        used  2165h (  8549) of 10000h bytes   ( 13.0%)
    Data space           used   140h (   320) of   F38h bytes   (  8.2%)

make[2]: Leaving directory 'C:/DEE/Dimmer/PIC/PWM_LCD_AD/PWM_LCD_AD_prj.X'
[31mmcc_generated_files/i2c_host/src/mssp2.c:293:: advisory: (2098) indirect function call via a NULL pointer ignored[0m
[32mBUILD SUCCESSFUL (total time: 6s)[0m
